
|  |
| --- |
| **IPv6 Addressing configuration** |

1. **Editing line to /etc/sysconfig/network**

Networking\_IPV6=yes




1. **Assign GW and IP address on single interface as manually.**

#Editing line on below.


IPV6ADDR=2001:41c8:1:5076::3/64 --🡪(IPv6 addressing and netmask)

IPV6\_DEFAULTGW=2001:41c8:1:5076::1 --🡪(IPv6 GW)


IPV6INIT=yes



1. **services should be stop NetworkManager before start network service**




1. **Identify IPv6 address on system.**

****

1. **check IPv6 is working or not by using pinging**

#ping6 2001:41c8:1:5076::3

****